*****************************************************************************
*                                                                           *
* All network interfaces are down at boot by default.                       *
* For GUI network manager, type "sudo rc-service NetworkManager start".     *
* Or you can type "sudo dhcpcd ethX" to setup your network interface.       *
*                                                                           *
* If you are running live USB, there are many ways to save changes:         *
* You can run "flushchanges" as root to automatically save any              *
*     changes made since boot.                                              *
* You can run "makemo category/package" as root to install a new package    *
*     which will be available now and after reboot.                         *
*                                                                           *
* Pentoo Bug Tracker: https://github.com/pentoo/pentoo-overlay/issues       *
* Update using "sudo pentoo-updater" command.                               *
*                                                                           *
*****************************************************************************

