diff -Naur /var/tmp/portage/net-wireless/compat-wireless-2.6.35_rc2-r1/work/compat-wireless-2.6.35-rc2/config.mk /usr/src/compat-wireless-2.6.35-rc2/config.mk
--- /var/tmp/portage/net-wireless/compat-wireless-2.6.35_rc2-r1/work/compat-wireless-2.6.35-rc2/config.mk	2010-06-12 01:28:31.000000000 -0400
+++ /usr/src/compat-wireless-2.6.35-rc2/config.mk	2010-06-12 01:35:32.000000000 -0400
@@ -172,7 +172,7 @@
 ifneq ($(CONFIG_PCI),)
 
 CONFIG_ATH5K=m
-# CONFIG_ATH5K_DEBUG=y
+CONFIG_ATH5K_DEBUG=y
 CONFIG_ATH9K_HW=m
 CONFIG_ATH9K=m
 # Note: once ath9k_htc is added we'll have to move
@@ -183,7 +183,7 @@
 
 
 CONFIG_IWLWIFI=m
-# CONFIG_IWLWIFI_DEBUG=y
+CONFIG_IWLWIFI_DEBUG=y
 # CONFIG_IWLWIFI_DEBUGFS=y
 # CONFIG_IWLWIFI_DEVICE_TRACING=y
 CONFIG_IWLAGN=m
@@ -202,30 +202,30 @@
 CONFIG_B43_PHY_LP=y
 CONFIG_B43_NPHY=y
 # CONFIG_B43_FORCE_PIO=y
-# CONFIG_B43_DEBUG=y
+CONFIG_B43_DEBUG=y
 
 CONFIG_B43LEGACY=m
 CONFIG_B43LEGACY_HWRNG=y
 CONFIG_B43LEGACY_PCI_AUTOSELECT=y
 CONFIG_B43LEGACY_LEDS=y
-# CONFIG_B43LEGACY_DEBUG=y
+CONFIG_B43LEGACY_DEBUG=y
 CONFIG_B43LEGACY_DMA=y
 CONFIG_B43LEGACY_PIO=y
 
 # The Intel ipws
 CONFIG_LIBIPW=m
-# CONFIG_LIBIPW_DEBUG=y
+CONFIG_LIBIPW_DEBUG=y
 
 
 CONFIG_IPW2100=m
 CONFIG_IPW2100_MONITOR=y
-# CONFIG_IPW2100_DEBUG=y
+CONFIG_IPW2100_DEBUG=y
 CONFIG_IPW2200=m
 CONFIG_IPW2200_MONITOR=y
 CONFIG_IPW2200_RADIOTAP=y
 CONFIG_IPW2200_PROMISCUOUS=y
 CONFIG_IPW2200_QOS=y
-# CONFIG_IPW2200_DEBUG=y
+CONFIG_IPW2200_DEBUG=y
 # The above enables use a second interface prefixed 'rtap'.
 #           Example usage:
 #
@@ -242,7 +242,7 @@
 ifneq ($(CONFIG_SSB),)
 # Sonics Silicon Backplane
 CONFIG_SSB_SPROM=y
-# CONFIG_SSB_DEBUG=y
+CONFIG_SSB_DEBUG=y
 
 CONFIG_SSB_BLOCKIO=y
 CONFIG_SSB_PCIHOST=y
@@ -250,7 +250,7 @@
 ifneq ($(CONFIG_PCMCIA),)
 CONFIG_SSB_PCMCIAHOST=y
 endif
-# CONFIG_SSB_DEBUG=y
+CONFIG_SSB_DEBUG=y
 CONFIG_SSB_DRIVER_PCICORE=y
 endif
 
@@ -327,7 +327,7 @@
 # USB Drivers
 ifneq ($(CONFIG_USB),)
 CONFIG_ZD1211RW=m
-# CONFIG_ZD1211RW_DEBUG=y
+CONFIG_ZD1211RW_DEBUG=y
 
 # Sorry, rndis_wlan uses cancel_work_sync which is new and can't be done in compat...
 
@@ -433,7 +433,7 @@
 # iwmc3200wifi uses new netdev_ops api no supported by old kernel.
 ifndef CONFIG_COMPAT_KERNEL_29
 CONFIG_IWM=m
-# CONFIG_IWM_DEBUG=y
+CONFIG_IWM_DEBUG=y
 endif
 
 endif # end of SDIO driver list
@@ -447,7 +447,7 @@
 CONFIG_RT2X00_LIB_FIRMWARE=y
 CONFIG_RT2X00_LIB_CRYPTO=y
 CONFIG_RT2X00_LIB_LEDS=y
-# CONFIG_RT2X00_DEBUG=y
+CONFIG_RT2X00_DEBUG=y
 # CONFIG_RT2X00_LIB_DEBUGFS
 endif
 
@@ -461,7 +461,7 @@
 
 # Atheros
 CONFIG_ATH_COMMON=m
-# CONFIG_ATH_DEBUG=y
+CONFIG_ATH_DEBUG=y
 
 CONFIG_WL12XX=y
 CONFIG_WL1251=m
@@ -476,7 +476,7 @@
 CONFIG_LIBERTAS_THINFIRM=m
 CONFIG_LIBERTAS=m
 CONFIG_LIBERTAS_MESH=y
-# CONFIG_LIBERTAS_DEBUG=y
+CONFIG_LIBERTAS_DEBUG=y
 endif
 endif
 
