diff -Naur /var/tmp/portage/net-wireless/compat-wireless-2.6.35_rc2-r1/work/compat-wireless-2.6.35-rc2/config.mk /usr/src/compat-wireless-2.6.35-rc2/config.mk
--- /var/tmp/portage/net-wireless/compat-wireless-2.6.35_rc2-r1/work/compat-wireless-2.6.35-rc2/config.mk	2010-06-11 15:32:27.000000000 -0400
+++ /usr/src/compat-wireless-2.6.35-rc2/config.mk	2010-06-11 15:34:16.000000000 -0400
@@ -130,7 +130,7 @@
 CONFIG_COMPAT_MAC80211_RC_DEFAULT=minstrel
 CONFIG_MAC80211_RC_PID=y
 CONFIG_MAC80211_RC_MINSTREL=y
-CONFIG_MAC80211_LEDS=y
+CONFIG_MAC80211_LEDS=n
 
 # enable mesh networking too
 CONFIG_MAC80211_MESH=y
@@ -198,7 +198,7 @@
 ifneq ($(CONFIG_PCMCIA),)
 CONFIG_B43_PCMCIA=y
 endif
-CONFIG_B43_LEDS=y
+CONFIG_B43_LEDS=n
 CONFIG_B43_PHY_LP=y
 CONFIG_B43_NPHY=y
 # CONFIG_B43_FORCE_PIO=y
@@ -207,7 +207,7 @@
 CONFIG_B43LEGACY=m
 CONFIG_B43LEGACY_HWRNG=y
 CONFIG_B43LEGACY_PCI_AUTOSELECT=y
-CONFIG_B43LEGACY_LEDS=y
+CONFIG_B43LEGACY_LEDS=n
 # CONFIG_B43LEGACY_DEBUG=y
 CONFIG_B43LEGACY_DMA=y
 CONFIG_B43LEGACY_PIO=y
@@ -351,13 +351,13 @@
 
 CONFIG_P54_USB=m
 CONFIG_RTL8187=m
-CONFIG_RTL8187_LEDS=y
+CONFIG_RTL8187_LEDS=n
 
 CONFIG_AT76C50X_USB=m
 
 ifndef CONFIG_COMPAT_KERNEL_28
 CONFIG_AR9170_USB=m
-CONFIG_AR9170_LEDS=y
+CONFIG_AR9170_LEDS=n
 endif
 
 CONFIG_ATH9K_HTC=m
@@ -446,7 +446,7 @@
 CONFIG_RT2X00_LIB_HT=y
 CONFIG_RT2X00_LIB_FIRMWARE=y
 CONFIG_RT2X00_LIB_CRYPTO=y
-CONFIG_RT2X00_LIB_LEDS=y
+CONFIG_RT2X00_LIB_LEDS=n
 # CONFIG_RT2X00_DEBUG=y
 # CONFIG_RT2X00_LIB_DEBUGFS
 endif
@@ -457,7 +457,7 @@
 
 # p54
 CONFIG_P54_COMMON=m
-CONFIG_P54_LEDS=y
+CONFIG_P54_LEDS=n
 
 # Atheros
 CONFIG_ATH_COMMON=m
